Edison configuration commands

configure\_edison –setup

Mraa library:

Mraa.Gpio(pin number)

Variablename.dir(mraa.DIR\_Direction) ==IN / OUT

Variablename.write(1/0) == writes logic level to an out pin

192.168.1.191

36274aa4a30dbf60ad4bd3f724517003 hash id